QSPI Communication between MC and SBC

In the Doc

info about QSPI module in the MC

info about SBC SPI interface

How communication happens between master (MC) and slave (SBC)

**SBC SPI**